                ********************************************
                *                                          *
                *    Windows Printer Drivers Setup Disk    *
                *                                          *
                ********************************************

Thank you for purchasing our product.

You have just opened the README.TXT file. It contains
information about the installation of the printer driver that
comes with your package.

*** Very important: ***
 1. Please don't overwrite the files of "UNIDRV.DLL" and "ICONLIB.DLL" to your
    windows system while installing this driver.


Printer Driver Installation Guide:
==================================
There are six Windows platforms supported by the this driver disk.  Each driver
resides in different directory described as follows:

        Platform                        Directory
        --------                        ---------
        Windows 98                        WIN98
        Windows 2000                      WIN2000
        Windows XP			  WinXP
        Windows 2003 Server	          Win2003
	Windiws Vista                     WinVista

You can run the setup application to install printer driver automatically in all of the above 
six Windows platforms, or use Windows "Add Printer" wizard to complete the installation.
The process will be as following,


Installing Windows 98 Printer Driver:

 1.     Select the Settings entry from the Start menu.
 2.     Select the Printers entry from the Settings menu.
 3.     Double-click the "Add" Printer icon.
 4.     Click the "Next" button.
 5.     Select which port your printer is connected.
 6.     Click the "Next" button.
 7.     Click the "Have Disk" button.
 8.     Put the Driver Disk into the drive A: (or B:, C:).
 9.     Click the "OK" button.
10.     Change directories to Win98.
11.     Highlight the corresponding printer driver name.
12.     Click the "Next" button.
13.     Highlight the corresponding printer port.
14.     Click the "Configure Port" button if you need to configure your port
        settings.
15.     Click the "Next" button.
16.     Click the "Next" button.
17.     Choose "No" without printing a test page or
               "Yes" with printing a test page.
18.     Click the "Finish" button.


Installing Windows 2000 Printer Driver:

 1.     Select the Settings entry from the Start menu.
 2.     Select the Printers entry from the Settings menu.
 3.     Double-click the "Add" Printer icon.
 4.     Click the "Next" button.
 5.     Select which port your printer is connected.
 6.     Click the "Next" button.
 7.     Click the "Have Disk" button.
 8.     Put the Driver Disk into the drive A: (or B:, C:).
 9.     Change directories to Win2000.
10.     Click the "OK" button.
11.     Highlight the corresponding printer driver name.
12.     Click the "Next" button.
13.     Highlight the corresponding printer port.
14.     Click the "Configure Port" button if you need to configure your port
        settings.
15.     Click the "Next" button.
16.     Click the "Next" button.
17.     Choose "No" without printing a test page or
               "Yes" with printing a test page.
18.     Click the "Finish" button.


Installing Windows XP/2003 Printer Driver:

 1.     Select the Settings entry from the Start menu.
 2.     Click the "printer and fax" settings entry menu.
 3.     Click the "Add Printer" icon from printer job of settings dialogue.
 4.     Click the "Next" button.
 5.     Select "Check Radio" to connect this computer to local printer without auto-detection.
 6.     Select which port your printer is connected.
 7.     Click the "Next" button.
 8.     Click the "Have Disk" button.
 9.     Put the Driver Disk into the drive A: (or B:, C:).
10.     Change directories to WinXP/Win2003.
11.     Click the "OK" button.
12.     Highlight the corresponding printer driver name.
13.     Click the "Next" button.
14.     Highlight the corresponding printer port.
15.     Click the "Configure Port" button if you need to configure your port
        settings.
16.     Click the "Next" button.
17.     Click the "Next" button.
18.     Choose "No" without printing a test page or
               "Yes" with printing a test page.
19.     Click the "Finish" button.

Installing Windows Vista Printer Driver:
1.     Select the Settings entry from the Start menu.
2.     Click the "Printers" settings entry menu.
3.     Right click the mouse and select the "Run as admnistrator" and then select the "Add Printer...".
4.     In the "User Access Control" Panel, select the "Continue".
5.     Select the "Add a local printer".
6.     Select which port your printer is connected.
7.     Click the "Have Disk" button.
8.     Change directories to WinVista for New model F1 and later model.
       or
       Change directories to WinVista\3 inch mode for old model.
                          to WinVista\4 inch mode
                          to WinVista\6 inch mode
9.     Highlight the corresponding printer driver name.
10.    Click the "Next" button.
11.    Confirm the printer name and click the "Next" button.
12.    If the "Windows Security" dialog is popped up, please don't care and select the "Install this driver software anyway".
13.    Click the "Yes" button in the dialog called as "The Printer Driver Change".
14.    The Windows Vista will perform the restart process.

Installing usb plug and play printer driver for the above operating system:
Printer Firmware versions fit for Label Dr200 ver 1.4.00 or later.
1.     Plug usb cable and turn on printer.
2.     Pop a "Found New Hardware Wizard" window.
3.     Select "install from a list or specific location(Advanced)".
4.     Click the "Next" button.
5.     Select "Search for the best driver in these locations."
6.     Check "Include this location in the search:" and browse the printer driver location.
7.     Click the "Next" button.
8.     Click the "Finish" button.
9.     Restart computer.

Release Notice:
===============
Ver 1.2.20
 1. In this version, we fixed the bug of control code for transferring to
    direct thermal mode of printer in Win95 platform.
 2. Add Win98 installation information file.
Ver 1.2.21
 1. In this version, we modified the limit of paper size to 8 inch for
    maximal width and 43 inch for maximal length in Win95, Win98 and
    NT operation system.
Ver 1.2.22
 1. In this version, we modified the environment parameters to avoid printing
    error in old NT 4.0 Germany version operation system.
 2. Add a sub-directory for installation of Traditional Chinese Windows version
    to avoid the UI page overlay between Traditional Chinese and English
    Windows version.
Ver 1.2.23
 1. Rename the develop identification code for mini-driver in Windows NT 4.0
    operation system.
Ver 1.2.24
 1. Add the utility to set some special parameters for PPLA printer language.
    Please read the readme file in "Utility" sub-directory for more
    installation information.
Ver 1.2.31
 1. Support Windows 2000 printer driver installation.
 2. Windows NT 3.51 and DOS commands generator will have not been included
    after this version.
 3. Separate printer driver into four models from original "Label Dr. 200".
Ver 1.2.41
 1. Modify the maximum printable label width to 168mm for 6 inch printer model.
 2. Modify printer driver to support bidirectional text printing, especially support the Arabic
    Windows version.
 3. Support Windows XP printer driver installation.
 4. Remove printer utility software from this driver disk. Please contact your vender for  
    support. 
Ver 1.3.00
 1. Add "Tear off" function in "Options" setting group of Windows printer driver.
 2. Add GDI commands to support new printers' modeles with centered paper guide. 
Ver 1.3.11    
 1. Support Windows XP printer driver installation.
Ver 1.3.12
 1. Add USB printer driver for Win 98, Win2000, WinXP.
 2. Add bi-direction communication for USB port.
Ver 1.3.13
 1. Support Windows 2003 Server printer driver installation.
 2. Add auto-install function.(only support for Win 98/2000/XP and 2003 Server)
Ver 1.3.14
 1. modify maximal printing width of 6 inch drive as 164mm.
Ver 1.3.15
 1. Modify the printer drivers build environment for Windows 2000 and Windows XP to meet the advanced 
    API function calls which are used in some third party software applications.
Ver 1.3.20
 This modification is for Windows 2000, Windows 2003 and Windows XP only, the other operation systems keep the previous versions.
 1. Add customer defined paper size function.
 2. Do not force to restart PC after driver installing.
 3. Add driver revision information.
Ver 1.4.00
 This modification is for Windows 2000, Windows 2003 and Windows XP only, the other operation systems keep the previous versions.
 1. Modify poor printing when printing a gray scale picture.
 2. Determine the max paper size according to gpd file.
 3. Auto-install show dialog to browse files when the system files do not find.
 4. Add plug and play settings for models with USB interface.

Ver PrinterDriver200_32-V5.00
 This modification is for Windows Vista only, the other operation systems keep the previous versions.
 1. Add the Vista support.

Ver PrinterDriver200_32/64-V5.01
 This modification is for Windows 98, Windows 2000, Windows 2003 ,Windows XP, and Windows Vista.
 1. Add the new model "Argox F1 (203 dpi)"

Ver PrinterDriver200_32/64-V5.02
 This modification is for Windows 98, the other operation systems keep the previous versions.
 1. Add the re-start mechanism for manual and automatic install.
 2. Add the USB PnP support.

Ver PrinterDriver200-V5.03
 1. Add new models, have:
    "Argox Inc. A-200 series PPLB", 
    "Argox Inc. OS-214 plus series PPLA/B", 
    "Argox Inc. R-400plus series PPLA/B/Z",
    "Argox Inc. X-1000V series PPLA/B",
    "Argox Inc. X-1000VL series PPLA/B",
    "Argox Inc. X-2000V series PPLA/B/Z"
    These models have USB port and the PID are different for all.
 2. Support Windows 2003 64bits printer driver installation.
 3. The version can setup in windows 32/64 bits version.

TRADEMARKS
==========
All trademark or brand names mentioned are properties
of their respective companies.


============END==========
